

* **********   FILTER SUBCKTS   ********

*   Filter Designer 6.3 - MicroSim Corp.

*   Design File Name: c:\st5\39a\kauer1.cir
*   Order:            3
*   Data type:        Continous
*   Function:         High Pass
*   Approximation:    Elliptic     

*   Specification:   Pass band cutoff:    400.0000 Hz
*                    Stop band cutoff:    250.0000 Hz
*                    Pass band ripple:      1.0000 dB
*                    Stop band atten.:     20.0000 dB
*                    Gain:                  0.0000 dB

*   Circuit Implementation: Biquad MLF 

.SUBCKT kauer1 IN OUT AGND
RIN IN 1 1
 X1 1 2 AGND LIN/STG
+  PARAMS:  C1VAL=     1.000e-8  C2VAL=     1.000e-8
+           R1VAL=    1.000e+20  R2VAL=     2.288e+4
 X2 2 3 AGND MLFBQ/STG
+  PARAMS:  C1VAL=    10.000e-9  C2VAL=    10.000e-9
+           R1VAL=     1.560e+4  R2VAL=     7.554e+4
+           R3VAL=     2.106e+4  R4VAL=     1.128e+5
+           R5VAL=      1.0e+20  R6VAL=     3.980e+4
+           R7VAL=     3.979e+4  R8VAL=     4.421e+3
ROUT 3 OUT 1
ROUTGND OUT AGND 1E12
.ENDS
