
**** 05/01/04 16:15:45 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * E:\Files\Technical University\TES\UPR 3\4.sch


 ****     CIRCUIT DESCRIPTION


******************************************************************************




* Schematics Version 9.2
* Sat May 01 16:15:44 2004



** Analysis setup **
.DC LIN I_I3 0 50u 200n 
.OP 


* From [PSPICE NETLIST] section of C:\Program Files\Orcad\PSpice\PSpice.ini:
.lib "E:\Files\Technical University\ASH\Project\OnSemiconductorDiscreteModels\Mje15030.lib"
.lib "E:\Files\Technical University\ASH\Project\OnSemiconductorDiscreteModels\Mje15031.lib"
.lib "E:\Files\Technical University\ASH\Project\OnSemiconductorDiscreteModels\Mje15035.lib"
.lib "E:\Files\Technical University\TES\UPR 6\UserLib\FILTERS.LIB"
.lib "E:\Files\Technical University\TES\UPR 6\UserLib\BB_new.lib"
.lib "E:\Files\Technical University\ASH\Project\OnSemiconductorDiscreteModels\Mje15034.lib"
.lib "nom.lib"

.INC "4.net"



**** INCLUDING 4.net ****
* Schematics Netlist *



V_Vce         $N_0001 0 20V
Q_Q1         $N_0001 $N_0002 0 Q2N3904
I_I3         $N_0002 0 DC 49.9u AC 10u
+SIN 0 10u 1k 0 0 0

**** RESUMING 4.cir ****
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 


.END

**** 05/01/04 16:15:45 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * E:\Files\Technical University\TES\UPR 3\4.sch


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N3904         
               NPN             
          IS    6.734000E-15 
          BF  416.4          
          NF    1            
         VAF   74.03         
         IKF     .06678      
         ISE    6.734000E-15 
          NE    1.259        
          BR     .7371       
          NR    1            
          RB   10            
          RC    1            
         CJE    4.493000E-12 
         MJE     .2593       
         CJC    3.638000E-12 
         MJC     .3085       
          TF  301.200000E-12 
         XTF    2            
         VTF    4            
         ITF     .4          
          TR  239.500000E-09 
         XTB    1.5          
          CN    2.42         
           D     .87         


**** 05/01/04 16:15:45 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * E:\Files\Technical University\TES\UPR 3\4.sch


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


($N_0001)   20.0000                   ($N_0002)-21.15E+06                   




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_Vce       -3.441E-05

    TOTAL POWER DISSIPATION   6.88E-04  WATTS


**** 05/01/04 16:15:45 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * E:\Files\Technical University\TES\UPR 3\4.sch


 ****     OPERATING POINT INFORMATION      TEMPERATURE =   27.000 DEG C


******************************************************************************






**** BIPOLAR JUNCTION TRANSISTORS


NAME         Q_Q1      
MODEL        Q2N3904   
IB          -2.87E-05 
IC           3.44E-05 
VBE         -2.12E+07 
VBC         -2.12E+07 
VCE          2.00E+01 
BETADC      -1.20E+00 
GM          -2.70E-13 
RPI          4.16E+14 
RX           1.00E+01 
RO           3.50E+06 
CBE          5.26E-14 
CBC          1.83E-14 
CJS          0.00E+00 
BETAAC      -1.13E+02 
CBX/CBX2     0.00E+00 
FT/FT2      -6.07E-01 



          JOB CONCLUDED

          TOTAL JOB TIME             .12
