

* **********   FILTER SUBCKTS   ********

*   Filter Designer 6.3 - MicroSim Corp.

*   Design File Name: D:\st11\46b\net.cir
*   Order:            4
*   Data type:        Continous
*   Function:         Low Pass
*   Approximation:    Chebyshev     

*   Specification:   Pass band cutoff:     2.0000K Hz
*                    Stop band cutoff:     3.0000K Hz
*                    Pass band ripple:      3.0000 dB
*                    Stop band atten.:     20.0000 dB
*                    Gain:                  0.0000 dB

*   Circuit Implementation: Basic MLF 

.SUBCKT net IN OUT AGND
RIN IN 1 1
 X1 1 2 AGND MLFLP/STG
+  PARAMS:  C1VAL=    10.000e-9  C2VAL=    5.000e-10
+           R1VAL=     3.487e+5  R2VAL=     2.934e+5
+           R3VAL=     2.202e+4
 X2 2 3 AGND MLFLP/STG
+  PARAMS:  C1VAL=    10.000e-8  C2VAL=    2.000e-10
+           R1VAL=     7.742e+4  R2VAL=     6.514e+4
+           R3VAL=     5.382e+3
ROUT 3 OUT 1
ROUTGND OUT AGND 1E12
.ENDS
