("FILE_TYPE"	"PMAP File"
    ("devices"
        ("VDC")
        ("LM324"
            ("info"
                ("spice_dsg"	"X")
            )
            ("smoke"
                ("max_ops_desc"
                    ("IPLUS"
                        ("description"	"Max input current(+)")
                        ("unit"	"A")
                    )
                    ("IMINUS"
                        ("description"	"Max input current(-)")
                        ("unit"	"A")
                    )
                    ("IOUT"
                        ("description"	"Max output current")
                        ("unit"	"A")
                    )
                    ("VDIFF"
                        ("description"	"Max differential VIN")
                        ("unit"	"V")
                    )
                    ("VSMAX"
                        ("description"	"Max supply volt diff")
                        ("unit"	"V")
                    )
                    ("VSMIN"
                        ("description"	"Min supply volt diff")
                        ("unit"	"V")
                    )
                    ("VCCMAX"
                        ("description"	"Max pos supply volt")
                        ("unit"	"V")
                    )
                    ("VEEMAX"
                        ("description"	"Max neg supply volt")
                        ("unit"	"V")
                    )
                    ("VPMAX"
                        ("description"	"Max inp volt(+)")
                        ("unit"	"V")
                    )
                    ("VPMIN"
                        ("description"	"Min inp volt(+)")
                        ("unit"	"V")
                    )
                    ("VMMAX"
                        ("description"	"Max inp volt(-)")
                        ("unit"	"V")
                    )
                    ("VMMIN"
                        ("description"	"Min inp volt(-)")
                        ("unit"	"V")
                    )
                )
                ("pre_smoke"
                    ("NODE_POS"	"PIN")
                    ("NODE_NEG"	"NIN")
                    ("NODE_VCC"	"PVss")
                    ("NODE_VEE"	"NVss")
                    ("NODE_GND"	"0")
                    ("TERM_POS"	"-1")
                    ("TERM_NEG"	"-2")
                    ("TERM_OUT"	"-3")
                    ("DERATE_TYPE"	"OPAMP")
                )
                ("max_ops")
                ("smoke_tests"
                    ("IMINUS"
                        ("test"	"current_test")
                        ("term"	"TERM_NEG")
                    )
                    ("IPLUS"
                        ("test"	"current_test")
                        ("term"	"TERM_POS")
                    )
                    ("IOUT"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_OUT")
                    )
                    ("VDIFF"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_POS")
                            ("NODE_NEG")
                        )
                    )
                    ("VMMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_NEG")
                            ("NODE_VCC")
                        )
                    )
                    ("VMMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_NEG")
                        )
                    )
                    ("VPMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_POS")
                            ("NODE_VCC")
                        )
                    )
                    ("VPMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_POS")
                        )
                    )
                    ("VCCMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VCC")
                            ("NODE_GND")
                        )
                    )
                    ("VEEMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_GND")
                            ("NODE_VEE")
                        )
                    )
                    ("VSMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VCC")
                            ("NODE_VEE")
                        )
                    )
                    ("VSMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_VCC")
                        )
                    )
                )
                ("device_max_ops"
                    ("VPMIN"	"0.3")
                    ("VMMIN"	"0.3")
                    ("IPLUS"	"50m")
                    ("IMINUS"	"50m")
                    ("IOUT"	"60m")
                    ("VDIFF"	"32")
                    ("VSMAX"	"32")
                    ("VSMIN"	"-3")
                    ("VPMAX"	"0")
                    ("VMMAX"	"0")
                    ("PDM"	"1.13")
                    ("VCCMAX"	"32")
                    ("VEEMAX"	"0")
                )
                ("device_pre_smoke"
                    ("TERM_POS"	"+")
                    ("TERM_NEG"	"-")
                    ("TERM_OUT"	"OUT")
                    ("NODE_POS"	"+")
                    ("NODE_NEG"	"-")
                    ("NODE_GND"	"0")
                    ("NODE_VCC"	"V+")
                    ("NODE_VEE"	"V-")
                    ("DERATE_TYPE"	"OPAMP")
                )
            )
        )
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("GAIN")
        ("C"
            ("info"
                ("spice_dsg"	"C")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("IC"
                        ("value"	"0")
                    )
                    ("TC"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("TERM_A"	"-1")
                    ("DERATE_TYPE"	"CAP")
                )
                ("max_ops"
                    ("CV"	"VOLTAGE")
                    ("CI"	"CURRENT")
                    ("SLP"	"SLOPE")
                    ("TBRK"	"KNEE")
                    ("TMAX"	"MAX_TEMP")
                )
                ("smoke_tests"
                    ("CV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("CI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_A")
                    )
                )
                ("device_max_ops")
            )
        )
    )
    ("instances"
        ("V6"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V6")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("U2A"
            ("device_name"	"LM324")
            ("pspice_path"	"X_U2A")
            ("level"	"0")
        )
        ("U1A"
            ("device_name"	"LM324")
            ("pspice_path"	"X_U1A")
            ("level"	"0")
        )
        ("V5"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V5")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"820")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("V4"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V4")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R6"
            ("device_name"	"R")
            ("pspice_path"	"R_R6")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"510")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("V2"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("U5A"
            ("device_name"	"LM324")
            ("pspice_path"	"X_U5A")
            ("level"	"0")
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"820")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("V9"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V9")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("R4"
            ("device_name"	"R")
            ("pspice_path"	"R_R4")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("GAIN1"
            ("device_name"	"GAIN")
            ("pspice_path"	"E_GAIN1")
            ("level"	"0")
            ("model_params"
                ("GAIN"
                    ("value"	"-1")
                    ("pspice_param"	"GAIN")
                )
            )
        )
        ("R5"
            ("device_name"	"R")
            ("pspice_path"	"R_R5")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("U4A"
            ("device_name"	"LM324")
            ("pspice_path"	"X_U4A")
            ("level"	"0")
        )
        ("V3"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V3")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"5V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("R7"
            ("device_name"	"R")
            ("pspice_path"	"R_R7")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("U3A"
            ("device_name"	"LM324")
            ("pspice_path"	"X_U3A")
            ("level"	"0")
        )
        ("R8"
            ("device_name"	"R")
            ("pspice_path"	"R_R8")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R15"
            ("device_name"	"R")
            ("pspice_path"	"R_R15")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R9"
            ("device_name"	"R")
            ("pspice_path"	"R_R9")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"500")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("C8"
            ("device_name"	"C")
            ("pspice_path"	"C_C8")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"10u")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R10"
            ("device_name"	"R")
            ("pspice_path"	"R_R10")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("C1"
            ("device_name"	"C")
            ("pspice_path"	"C_C1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"5u")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R11"
            ("device_name"	"R")
            ("pspice_path"	"R_R11")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R12"
            ("device_name"	"R")
            ("pspice_path"	"R_R12")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("C2"
            ("device_name"	"C")
            ("pspice_path"	"C_C2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"2u")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R13"
            ("device_name"	"R")
            ("pspice_path"	"R_R13")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R14"
            ("device_name"	"R")
            ("pspice_path"	"R_R14")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("C3"
            ("device_name"	"C")
            ("pspice_path"	"C_C3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.2u")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R16"
            ("device_name"	"R")
            ("pspice_path"	"R_R16")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("GAIN2"
            ("device_name"	"GAIN")
            ("pspice_path"	"E_GAIN2")
            ("level"	"0")
            ("model_params"
                ("GAIN"
                    ("value"	"-1")
                    ("pspice_param"	"GAIN")
                )
            )
        )
    )
)
