msp430xG46x_1.asm - Software Toggle P1.0
msp430xG46x_adc12_01.asm - ADC12, Sample A0, Set P5.1 if A0 > 0.5*AVcc
msp430xG46x_adc12_02.asm - ADC12, Using the Internal Reference
msp430xG46x_adc12_03.asm - ADC12, Sample A10 Temp, Set P5.1 if Temp ++ ~2C
msp430xG46x_adc12_04.asm - ADC12, Extend Sampling Period with SHT Bits
msp430xG46x_adc12_05.asm - ADC12, Using an External Reference
msp430xG46x_adc12_06.asm - ADC12, Repeated Sequence of Conversions
msp430xG46x_adc12_07.asm - ADC12, Repeated Single Channel Conversions
msp430xG46x_adc12_08.asm - ADC12, Using 10 External Channels for Conversion
msp430xG46x_adc12_09.asm - ADC12, Sequence of Conversions (non-repeated)
msp430xG46x_adc12_10.asm - ADC12, Sample A10 Temp and Convert to oC and oF
msp430xG46x_bt_01.asm -	Basic Timer, Toggle P5.1 Inside ISR, 32kHz ACLK
msp430xG46x_clks_02.asm - FLL+, Output 32kHz Xtal + HF Xtal + Internal DCO
msp430xG46x_compA_01.asm - Comparator A, Poll input CA0, result in P5.1
msp430xG46x_compA_02.asm - Comparator A, Poll input CA0, CA exchange, result in P5.1
msp430xG46x_compA_04.asm -  Comparator A, Poll input CA0, result in P5.1
msp430xG46x_compA_05.asm - Comparator A, Poll input CA0, interrupt triggered
msp430xG46x_dac12_01.asm - DAC12_0, Output 1.0V on DAC0
msp430xG46x_dac12_02.asm - DAC12_1, Output 2.0V on DAC1
msp430xG46x_dac12_03.asm- DAC12_0, Output Voltage Ramp on DAC0
msp430xG46x_dma_01.asm - DMA0, Repeated Burst to-from RAM, Software Trigger
msp430xG46x_dma_02.asm - DMA0, Repeated Block to P1OUT, TACCR2 Trigger
msp430xG46x_dma_04.asm - DMA0, Block Mode UART1 9600, ACLK
msp430xG46x_dma_05.asm - DMA0, Repeated Blk to DAC0, Sine Output, TACCR1, DCO
msp430xG46x_dma_06.asm - DMA2, Rpt'd Blk to DAC1, 8-Bit Sine, TBCCR2, DCO
msp430xG46x_dma_07.asm - DMA0/1, Rpt'd Blk to DAC12_0/1, Sin/Cos, TACCR1, XT2
msp430xG46x_dma_08.asm - DDMA0, Rpt'd Block, I2C Master Intf. to DAC8571, DCO
msp430xG46x_dma_09.asm - DMA0, ADC12 A10 Block Xfer to RAM, TBCCR1, DCO
msp430xG46x_fll_01.asm - FLL+, Runs Internal DCO at 2.45MHz
msp430xG46x_fll_02.asm -  FLL+, Runs Internal DCO at 8MHz
msp430xG46x_hfxt2.asm -  FLL+, MCLK Configured to Operate from XT2 HF XTAL
msp430xG46x_lpm3.asm - Basic Clock, LPM3 Using WDT ISR, 32kHz ACLK
msp430xG46x_MPY_01.asm - 16x16 Unsigned Multiply
msp430xG46x_MPY_02.asm - 8x8 Unsigned Multiply
msp430xG46x_MPY_03.asm - 16x16 Signed Multiply
msp430xG46x_MPY_04.asm - 8x8 Signed Multiply
msp430xG46x_MPY_05.asm - 16x16 Unsigned Multiply Accumulate
msp430xG46x_MPY_06.asm - 8x8 Unsigned Multiply Accumulate
msp430xG46x_MPY_07.asm - 16x16 Signed Multiply Accumulate
msp430xG46x_MPY_08.asm - 8x8 Signed Multiply Accumulate
msp430xG46x_oa_01.asm - OA0, Comparator Mode
msp430xG46x_oa_02.asm - OA0, Comparator in General-Purpose Mode
msp430xG46x_oa_03.asm - OA0, General-Purpose Mode
msp430xG46x_oa_04.asm - OA0, Inverting PGA Mode
msp430xG46x_oa_05.asm - OA0, Non-Inverting PGA Mode
msp430xG46x_oa_06.asm - OA0, Unity-Gain Buffer Mode
msp430xG46x_oa_07.asm - OA1, Comparator Mode
msp430xG46x_oa_08.asm - OA1, Comparator in General-Purpose Mode
msp430xG46x_oa_09.asm - OA1, Inverting PGA Mode
msp430xG46x_oa_10.asm - OA1, Non-Inverting PGA Mode
msp430xG46x_oa_11.asm - OA1, Unity-Gain Buffer Mode
msp430xG46x_oa_12.asm - 3-Amp Differential Amplifier with OA0, OA1, and OA2
msp430xG46x_oa_13.asm - 3-Amp Differential Amplifier with OA1, OA2, and OA0
msp430xG46x_oa_14.asm - 3-Amp Differential Amplifier with OA2, OA0, and OA1
msp430xG46x_OF_LFXT1_nmi.asm - LFXT1 Oscillator Fault Detection
msp430xG46x_OF_XT2.asm - XT2 Oscillator Fault Detection
msp430xG46x_P1_01.asm - Software Poll P1.4, Set P5.1 if P1.4 = 1
msp430xG46x_P1_02.asm - Software Port Interrupt on P1.4 from LPM4
msp430xG46x_P1_05.asm - Write a byte to Port 1
msp430xG46x_P7_05.asm - Write a byte to Port 7
msp430xG46x_P8_05.asm - Write a byte to Port 8
msp430xG46x_PA_05.asm - Write a word to Port A
msp430xG46x_PB_05.asm - Write a word to Port B
msp430xG46x_rtc_01.asm - Real Time Clock, Toggle P5.1 Inside ISR, 32kHz ACLK;and send Time via UART
msp430xG46x_rtc_02.asm - Real Time Clock, Toggle P5.1 Inside ISR, 32kHz ACLK
msp430xG46x_ta_01.asm - Timer_A, Toggle P5.1, TACCR0 Cont. Mode ISR, DCO SMCLK
msp430xG46x_ta_02.asm - Timer_A, Toggle P5.1, TACCR0 Up Mode ISR, DCO SMCLK
msp430xG46x_ta_03.asm - Timer_A, Toggle P5.1, Overflow ISR, DCO SMCLK
msp430xG46x_ta_04.asm - Timer_A, Toggle P5.1, Overflow ISR, 32kHz ACLK
msp430xG46x_ta_05.asm - Timer_A, Toggle P5.1, TACCR0 Up Mode ISR, 32kHz ACLK
msp430xG46x_ta_08.asm - Timer_A, Toggle P1.0,P1.2 & P2.0 Cont. Mode ISR, 32kHz ACLK
msp430xG46x_ta_11.asm - Timer_A, Toggle P1.0/TA0, Up Mode, 32kHz ACLK
msp430xG46x_ta_13.asm - Timer_A, Toggle P1.0/TA0, Up/Down Mode, DCO SMCLK
msp430xG46x_ta_17.asm - Timer_A, PWM TA1-2 Up Mode, 32kHz ACLK
msp430xG46x_ta_19.asm - Timer_A, PWM TA1-2, Up/Down Mode, 32kHz ACLK
msp430xG46x_tb_01.asm - Timer_B, Toggle P5.1, TBCCR0 Cont. Mode ISR, DCO SMCLK
msp430xG46x_tb_02.asm - Timer_B, Toggle P5.1, TBCCR0 Up Mode ISR, DCO SMCLK
msp430xG46x_tb_04.asm - Timer_B, Toggle P5.1, Overflow ISR, 32kHz ACLK
msp430xG46x_tb_05.asm - Timer_B, Toggle P5.1, TBCCR0 Up Mode ISR, 32kHz ACLK
msp430xG46x_tb_10.asm - Timer_B, PWM TB1-6, Up Mode, DCO SMCLK
msp430xG46x_usart1_19200.asm - USART1, Ultra-Low Pwr UART 19200 Echo ISR, 32kHz ACLK
msp430xG46x_usart1_spi0_09.asm - USART1, SPI 3-Wire Master Incremented Data
msp430xG46x_usart1_spi0_10.asm - USART1, SPI 3-Wire Slave Data Echo
msp430xG46x_usart1_spi1_01.asm - USART1, SPI Interface to TLC549 8-Bit ADC
msp430xG46x_usart1_uart_115k.asm - USART1, 115200 UART Echo ISR, DCO SMCLK
msp430xG46x_usart1_uart_2400.asm - USART1, Ultra-Low Pwr UART 2400 Echo ISR, 32kHz ACLK
msp430xG46x_usart1_uart_9600.asm - USART1, Ultra-Low Pwr UART 9600 Echo ISR, 32kHz ACLK
msp430xG46x_uscia0_duplex_9600.asm - USCI_A0, UART 9600 Full-Duplex Transceiver, 32K ACLK
msp430xG46x_uscia0_irda_01.asm - USCI_A0 IrDA External Loopback Test, 4MHz SMCLK
msp430xG46x_uscia0_irda_02.asm - USCI_A0 IrDA Monitor, 4MHz SMCLK
msp430xG46x_uscia0_irda_03.asm - USCI_A0 IrDA Physical Layer Comm, 4MHz SMCLK
msp430xG46x_uscia0_spi_09.asm - USCI_A0, SPI 3-Wire Master Incremented Data
msp430xG46x_uscia0_spi_10.asm - USCI_A0, SPI 3-Wire Slave Data Echo
msp430xG46x_uscia0_uart_115k.asm - USCI_A0, 115200 UART Echo ISR, DCO SMCLK
msp430xG46x_uscia0_uart_115k_lpm.asm - USCI_A0, 115200 UART Echo ISR, DCO SMCLK, LPM3
msp430xG46x_uscia0_uart_9600.asm - USCI_A0, Ultra-Low Pwr UART 9600 Echo ISR, 32kHz ACLK
msp430xG46x_uscib0_i2c_02.asm - USCI_B0 I2C Master Interface to PCF8574, Read/Write
msp430xG46x_uscib0_i2c_03.asm - USCI_B0 I2C Master Interface to DAC8571, Write
msp430xG46x_uscib0_i2c_08.asm - USCI_B0 I2C Master TX multiple bytes to MSP430 Slave
msp430xG46x_uscib0_i2c_09.asm - USCI_B0 I2C Slave RX multiple bytes from MSP430 Master
msp430xG46x_uscib0_i2c_10.asm - USCI_B0 I2C Master RX multiple bytes from MSP430 Slave
msp430xG46x_uscib0_i2c_11.asm - USCI_B0 I2C Slave TX multiple bytes to MSP430 Master
msp430xG46x_uscib0_spi_01.asm - USCI_B0, SPI Interface to TLC549 8-Bit ADC