
**** 01/12/10 01:22:45 ******* PSpice 16.0.0 (July 2006) ****** ID# 1665768 **

 ** Profile: "LAB_DIF1-time"  [ D:\Desktop\Dian\TU\tu work\analogova shemotehnika\analogova upr2\LAB_DIF1-PSpiceFiles\LAB_DIF1\time.s


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "time.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of D:\Programs\OrCad 16\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 5m 0 1u 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\LAB_DIF1.net" 



**** INCLUDING LAB_DIF1.net ****
* source LAB_DIF1
V_V1         +VCC 0 15V
V_V2         -VCC 0 -15V
C_C         N00125 VOUT  0,1n  
-------------------------$
ERROR -- Value may not be 0
X_U1         0 N00125 +VCC -VCC VOUT LM741
R_R2         N03464 N00125  1k  
V_V3         N03464 0  
+PULSE -2V 2V 0 1.6ms 0.4ms 0 2m
.PARAM  rvar=51k

**** RESUMING time.cir ****
.END
