Microchip MPLAB IDE v 8.30
CCS PICC Compiler - PCWH v 4.088
Portable Edition
How To Install
------------------------------------------

1) Copy all files to any drive / folder. Don't copy
    the .rar files if you don't need the examples
    and documentation.

2) To configure CCS PICC inside the MPLAB IDE:

	a) Execute "MPLAB IDE.exe"
	b) Goto Project -> Set Language Tools Locations...
	c) Select CCS Compiler for PIC10/...
	d) Select Executables
	e) Select CCS C Compiler (ccsc.exe)
	f) Click in Browse ...
	g) Goto
	    C:\Program files\Picc\CCSC.exe          or
	    C:\Archivos de Programa\Picc\CCSC.exe   or
	    C:\<some dir>\Picc\CCSC.exe
	h) Press OK.

3) Enjoy!!


Note:
-------

This software has been portabilized with ThinApp of VmWare.
ThinApp stores the user configuration in the folder:

	C:\Documents and Settings\Username\Program Data\Thinstall\MPLAB v8.30 CCS v4.088
	C:\Documents and Settings\Username\Datos de programa\Thinstall\MPLAB v8.30 CCS v4.088
	C:\Documents and Settings\Username\<some dir>\Thinstall\MPLAB v8.30 CCS v4.088

If you delete this folder, you need to run again the point (2)
to (re)configure MPLAB IDE with CCS PICC.
